****

**PopUp WiFi Go HD**

Compact, powerful, high-availability WiFi unit with external ethernet port and battery compatibility.

**Quick Facts**

Runs two cellular providers concurrently.

CAPTIVATE compatible.

Crowd counting and presence analytics compatible

**Dimensions**

31 x 27 x 20 cm

5kg

**Router**

Multi-provider capable (1 x Telstra 1 x Optus)

200Mbps throughput

8 Load-balancing algorithms

Static IP capable

Cloud-managed

Medium-gain antennas for high 4G performance

16 VLANs

**Access Point**

50 concurrent users

CAPTIVATE compatible

2x2 MIMO

5Ghz and 2.4Ghz (5Ghz recommended)

Complies with all main WiFi security standards

Web content filtering

**Power**

Powered by standard Australian power plug

Battery power available via external 4 pin XLR connector.

Low power consumption (approx. 20 watts)

Compatible with generators

Tested and tagged

**Build**

Rugged hard case construction.

Splash resistant.

Approved to take as carry-on or checked baggage on planes.

Locked, can be opened by airport security (TSA approved)

4 pin XLR power inlet to connect to battery power.

Green power indicator light.

External Ethernet – CAT6A for connecting a network switch, direct client access or external WAN.